DIV2
FFmpeg-4 V2 (hacked MS MPEG-4 V2)
AVRN
Avid Motion JPEG
Y8
Simple grayscale video
DIV3
DivX ;-) MPEG-4 Low motion
T420
Toshiba YUV 4:2:0
DIV4
DivX ;-) MPEG-4 Fast motion
DIVF
DivX 4 Codec
V261
Lucent VX2000S
MPEGFILE
MPEG Video
DIV5
DivX ;-) MPEG-4
DIV6
DivX ;-) MPEG-4
VX2K
Lucent VX2000S Video Codec
HFYU
Huffman Lossless Codec YUV and RGB formats (with Alpha-channel)
CYUV
Creative Labs YUV 4:2:2
DMB1
Matrox Rainbow Runner hardware compression (Motion JPEG)
CPLA
Weitek YUV 4:2:0 Planar
HMRR
Rendition Motion Compensation Format
FRWT
Darim Vision Forward Motion JPEG
DMB2
Motion JPEG codec used by Paradigm
KMVC
Karl Morton Video Codec
FRWU
Darim Vision Forward Uncompressed
DSVD
Microsoft DirectShow DV
MMES
Matrox MPEG-2 I-frame
DPSC
DPS PAR Motion JPEG
ILVR
ITU H.263+ Codec
IJPG
Intergraph JPEG
CWLT
Microsoft Color WLT DIB
MWV1
Aware Motion Wavelets
M261
Microsoft H.261
V422
Vitec Multimedia YUV 4:2:2 as for UYVY but with different component ordering within the u_int32 macropixel
M263
Microsoft H.263
V655
Vitec Multimedia 16 bit YUV 4:2:2 (6:5:5) format
CYUY
ATI Technologies YUV
NVT0
Nvidia texture compression format
MTX8
Matrox codec
MDVD
Alex MicroDVD Video (hacked MS MPEG-4)
BTCV
Conexant Composite Video
NVT1
Nvidia texture compression format
NAVI
nAVI video codec (hacked MS MPEG-4)
MTX9
Matrox codec
3IV0
MPEG4-based codec 3ivx
NVT2
Nvidia texture compression format
FRWD
Darim Vision Forward Motion JPEG
AZPR
Quicktime Apple Video
AVDJ
Avid Motion JPEG
3IV1
MPEG4-based codec 3ivx
NVT3
Nvidia texture compression format
MSS1
Windows Screen Video
3IV2
MPEG4-based codec 3ivx
NVT4
Nvidia texture compression format
IYU2
24 bit format used in mode 2 of the IEEE 1394 Digital Camera 1.04 spec
NVT5
Nvidia texture compression format
CVID
Cinepak by Radius YUV 4:2:2
U263
UB Video StreamForce H.263
IYU1
12 bit format used in mode 2 of the IEEE 1394 Digital Camera 1.04 spec
ILVC
Intel Layered Video
FRWA
Darim Vision Forward Motion JPEG with Alpha-channel
ETVC
eTreppid Video Codec
IGOR
Power DVD
NUV1
NuppelVideo
MTX1
Matrox codec
NVS4
Nvidia texture compression format
MTX2
Matrox codec
DVSD
Sony Digital Video (DV) 525 lines at 29.97 Hz or 625 lines at 25.00 Hz
NVS5
Nvidia texture compression format
MTX3
Matrox codec
NVS2
Nvidia texture compression format
MTX4
Matrox codec
NVS3
Nvidia texture compression format
MTX5
Matrox codec
NVS0
Nvidia texture compression format
MTX6
Matrox codec
ICLB
CellB Videoconferencing Codec
ELK0
Else graphics card codec
NVS1
Nvidia texture compression format
MTX7
Matrox codec
CRAM
Microsoft Video 1
YUVP
YCbCr 4:2:2 extended precision 10-bits per component in Y0U0Y1V0 order
TLST
TeraLogic Motion Infraframe Codec B
Y411
YUV 4:1:1 Packed
PVW2
Pegasus Imaging Wavelet 2000
Y422
Direct copy of UYVY as used by ADS Technologies Pyro WebCam firewire camera
PGVV
Radius Video Vision Telecast (adaptive JPEG)
VIXL
miroVideo XL
VDOW
VDOLive (H.263)
Y211
Packed YUV format with Y sampled at every second pixel across each line and U and V sampled at every fourth pixel
EM2V
Etymonix MPEG-2 I-frame
X263
Xirlink H.263
SVQ3
Sorenson Video 3 (Apple Quicktime 5)
AP41
AngelPotion Definitive (hack MS MP43)
VDCT
Video Maker Pro DIB
VDOM
VDOnet VDOWave
SVQ1
Sorenson Video (Apple Quicktime 3)
PIMJ
Pegasus Imaging PICvideo Lossless JPEG
BT20
Conexant (ex Brooktree) ProSummer MediaStream
PHMO
Photomotion
YVYU
YUV 4:2:2 as for UYVY but with different component ordering within the u_int32 macropixel
WJPG
Winbond JPEG
VIVO
Vivo H.263
YUYV
Canopus YUV format
ULTI
IBM Corp. Ultimotion
IAN
Indeo 4 (RDX) Codec
SQZ2
Microsoft VXTreme Video Codec V2
DX50
DivX 5.0 codec
UCOD
ClearVideo (fractal compression-based codec)
BW10
Data Translation Broadway MPEG Capture/Compression
PDVC
Panasonic DV codec
DV50
Matrox DVCPRO50 codec
M4S2
Microsoft MPEG-4 (hacked MS MPEG-4)
TMIC
TeraLogic Motion Intraframe Codec 2
VIFP
Virtual Frame API codec (VFAPI)
SMSC
Radius proprietary codec
RGBA
Raw RGB with alpha
DV25
Matrox DVCPRO codec
XLV0
NetXL Inc. XL Video Decoder
SDCC
Sun Digital Camera Codec
XVID
XviD MPEG-4 codec
SMSD
Radius proprietary codec
VIDS
Vitec Multimedia YUV 4:2:2 codec
Y800
Simple grayscale video
DVC
MainConcept DV Codec
DIB
Full Frames (Uncompressed)
VDTZ
Darim Vision VideoTizer YUV
MP4S
Microsoft MPEG-4 (hacked MS MPEG-4)
VGPX
Alaris VGPixel Codec
MC12
ATI Motion Compensation Format
YUNV
A direct copy of YUY2 registered by NVidia to work around problems in some old codecs which did not like hardware which offered more than 2 YUY2 surfaces
MP4V
Microsoft MPEG-4 (hacked MS MPEG-4)
WHAM
Microsoft Video 1
SJPG
White Pine (ex Paradigm Matrix) Motion JPEG
WINX
Winnov Software Compression
TLMS
TeraLogic Motion Infraframe Codec A
SFMC
Crystal Net SFM Codec
SMSV
WorldConnect Wavelet Streaming Video
RUD0
Rududu video codec
RGBT
Uncompressed RGB with transparency
ZPEG
Metheus Video Zipper
TMOT
TrueMotion Video Compression
WBVC
Winbond W9960 codec
IV48
Intel Indeo Video 4.8
IV36
Intel Indeo Video 3.6
IV49
Intel Indeo Video 4.9
IV37
Intel Indeo Video 3.7
IV34
Intel Indeo Video 3.4
YVU9
Brooktree YVU9 Raw (YVU9 Planar)
IV35
Intel Indeo Video 3.5
IV32
Intel Indeo Video 3.2
CC12
Intel YUV12 Codec
STVA
ST CMOS Imager Data (Bayer)
RPZA
Apple Video 16 bit "road pizza"
IV33
Intel Indeo Video 3.3
VXSP
Lucent VX1000SP Video Codec
STVB
ST CMOS Imager Data (Nudged Bayer)
IV30
Intel Indeo Video 3
STVC
ST CMOS Imager Data (Bunched)
MJ2C
Morgan Multimedia JPEG2000 Compression
IV31
Intel Indeo Video 3.1
YUV8
Winnov Caviar YUV8
TVMJ
Field Encoded Motion JPEG (Targa emulation)
IV40
Intel Indeo Video 4.0
DVE2
DVE-2 Videoconferencing Codec
ABYR
Kensington codec
YUV9
Intel YUV9
VIV1
Vivo H.263
TSCC
TechSmith Screen Capture Codec
IV41
Intel Indeo Video 4.1
VIV2
Vivo H.263
IV50
Intel Indeo Video 5.0 Wavelet
IV42
Intel Indeo Video 4.2
IV43
Intel Indeo Video 4.3
BINK
Bink Video (RAD Game Tools) (256 color)
PIM2
Pegasus Imaging codec
IV44
Intel Indeo Video 4.4
IV45
Intel Indeo Video 4.5
MPEG
Chromatic MPEG 1 Video I Frame
IV46
Intel Indeo Video 4.6
IV38
Intel Indeo Video 3.8
PIM1
Pegasus Imaging codec
IV47
Intel Indeo Video 4.7
IV39
Intel Indeo Video 3.9
MRCA
FAST Multimedia MR Codec
CDVC
Canopus DV Codec
ZLIB
Lossless codec (ZIP compression)
UYVP
YCbCr 4:2:2 extended precision 10-bits per component in U0Y0V0Y1 order
TM2X
Duck TrueMotion 2X
WMV1
Windows Media Video 7
AASC
Autodesk Animator codec
WMV2
Windows Media Video 8
RLE8
Run length encoded 8bpp RGB image
AUR2
Aura 2 Codec - YUV 422
WMV3
Windows Media Video 9
GLZW
Motion LZW by gabest@freemail.hu
IR21
Intel Indeo 2.1
CLJR
Cirrus Logic YUV 4:1:1
MPGI
Sigma Design MPEG-1 I-frame
ANIM
Intel RDX
DIVX
OpenDivX (DivX 4.0 and later)
UYVY
YUV 4:2:2 (Y sample at every pixel, U and V sampled at every second pixel horizontally on each line)
TM2A
Duck TrueMotion Archiver 2.0
SV10
Sorenson Media Video R1
MPNG
Motion PNG codec
YUY2
YUV 4:2:2 as for UYVY but with different component ordering within the u_int32 macropixel
STVX
ST CMOS Imager Data (Extended)
YC12
Intel YUV12 Codec
WNV1
WinNow Videum Hardware Compression
VLV1
VideoLogic codec
STVY
ST CMOS Imager Data (Extended with Correction Data)
RT21
Intel Real Time Video 2.1
FVF1
Fractal Video Frame
RLE4
Run length encoded 4bpp RGB image
CHAM
WinNow Caviara Champagne
VCR8
ATI VCR 8.0
IUYV
Interlaced version of UYVY (line order 0, 2, 4,....,1, 3, 5....)
VCR9
ATI VCR 9.0
RV13
RealVideo codec
DXT1
DirectX Compressed Texture
ASV1
Asus Video V1
RV10
RealVideo codec
DXT2
DirectX Compressed Texture
ASV2
Asus Video V2
SPLC
Splash Studios ACM Audio Codec
DXT3
DirectX Compressed Texture
RV20
RealVideo G2
DXT4
DirectX Compressed Texture
QPEG
Q-Team QPEG 1.1
MRLE
Microsoft Run Length Encoding
DXT5
DirectX Compressed Texture
UYNV
A direct copy of UYVY registered by NVidia to work around problems in some old codecs which did not like hardware which offered more than 2 UYVY surfaces
RV30
RealVideo 8
PVEZ
Horizons Technology PowerEZ codec
VCR1
ATI VCR 1.0
AFLI
Autodesk Animator FLI (256 color)
VCR2
ATI VCR 2.0 (MPEG YV12)
VCR3
ATI VCR 3.0
VCR4
ATI VCR 4.0
FLJP
Field Encoded Motion JPEG (Targa emulation)
D261
H.261
VCR5
ATI VCR 5.0
SPIG
Radius Spigot
RVX
Intel RDX
ETV1
eTreppid Video Codec
CGDI
Camcorder Video (MS Office 97)
CFCC
Conkrete DPS Perception Motion JPEG
VCR6
ATI VCR 6.0
VP30
On2 (ex Duck TrueMotion) VP3
ETV2
eTreppid Video Codec
D263
H.263
VCR7
ATI VCR 7.0
PVMM
PacketVideo Corporation MPEG-4
VP31
On2 (ex Duck TrueMotion) VP3
RMP4
REALmagic MPEG-4 Video Codec
NT00
NewTek LigtWave HDTV YUV with Alpha-channel
MP42
Microsoft MPEG-4 V2
TV10
Tecomac Low-Bit Rate Codec
XMPG
XING MPEG (I frame only)
QPEQ
Q-Team QPEG 1.1
MP43
Microsoft MPEG-4 V3
MSVC
Microsoft Video 1
AFLC
Autodesk Animator FLC (256 color)
RGB
Full Frames (Uncompressed)
IY41
Interlaced version of Y41P (line order 0, 2, 4,....,1, 3, 5....)
LSVM
Vianet Lighting Strike Vmail (Streaming)
DVS1
DV compressed in SD (SDL)
AEMI
Array VideoONE MPEG1-I Capture
IYUV
Intel Indeo iYUV 4:2:0
JPGL
DIVIO JPEG Light for WebCams
IRAW
Intel YUV Uncompressed
CMYK
Common Data Format in Printing
IPDV
Giga AVI DV Codec
DPS0
DPS Reality Motion JPEG
CJPG
Creative Video Blaster Webcam Go JPEG
MSZH
Lossless codec (ZIP compression)
ASF0
Windows Media Video
DVX1
DVX1000SP Video Decoder
3IVX
MPEG4-based codec 3ivx
DVX2
DVX2000S Video Decoder
I420
Intel Indeo 4 H.263
DVX3
DVX3000S Video Decoder
AMPG
Array VideoONE MPEG
TR20
Duck TrueMotion RT 2.0
JPEG
Still Image JPEG DIB
SMC
Apple Graphics (SMC) codec (256 color)
RLE
Raw RGB with arbitrary sample packing within a pixel
H264
H.264
Y42T
Format as for UYVY but the lsb of each Y component is used to signal pixel transparency
YV12
ATI YVU12 4:2:0 Planar
TM20
Duck TrueMotion 2.0
HMCR
Rendition Motion Compensation Format
H265
H.265
MJPA
Pinnacle Motion JPEG with Alpha-channel
H266
H.266
Y41P
Conexant (ex Brooktree) YUV 4:1:1 Raw
MJPB
Motion JPEG codec
H267
H.267
TY2C
Trident Decompression Driver
H260
H.260
DVMA
Darim Vision DVMPEG
H261
H.261
H262
H.262
Y41T
Format as for Y41P but the lsb of each Y component is used to signal pixel transparency
RAW
Full Frames (Uncompressed)
H263
Intel ITU H.263
MJPG
IBM Motion JPEG including Huffman Tables
GWLT
Microsoft Greyscale WLT DIB
TY0N
Trident Decompression Driver
MCAM
ATI Motion Compensation Format
H268
H.268
DXTC
DirectX Texture Compression
H269
H.263 for POTS-based videoconferencing
DVHD
DV 1125 lines at 30.00 Hz or 1250 lines at 25.00 Hz
NTN1
Nogatech Video Compression 1
TY2N
Trident Decompression Driver
I263
Intel ITU H.263
DVCP
Sony Digital Video (DV)
LJPG
LEAD Motion JPEG Codec
BTVC
Conexant Composite Video
Y41B
YUV 4:1:1 Planar
ASVX
Asus Video 2.0
MPG4
Microsoft MPEG-4 V1
LEAD
LEAD Video Codec
ESCP
Eidos Technologies Escape codec
IAVS
interleaved audio and video stream
FVFW
ff MPEG-4 based on XviD codec
MPG2
FFmpeg-1
MPG3
Same as Low motion DivX MPEG-4
GPEG
Motion JPEG by gabest@freemail.hu (with floating point)
Y42B
YUV 4:2:2 Planar
S422
VideoCap C210 YUV Codec
EKQ0
Else graphics card codec
MPG1
FFmpeg-1
Q1.0
Q-Team QPEG 1.0
VX1K
Lucent VX1000S Video Codec
DUCK
True Motion 1.0
DIV1
FFmpeg-4 V1 (hacked MS MPEG-4 V1)
AURA
Aura 1 Codec - YUV 411
